{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":12,"n_cols":6,"rows_kept":12,"merged":[[9,0,10,0],[9,2,10,2],[9,3,10,3],[9,4,10,4],[9,5,10,5],[11,0,11,5]],"flags":["formulas_cached_only"]}
["序号","名称","规格型号","单位","数量","备注"]
[1,"智能化矿用液压移动列车组",null,"套",1]
[1.1,"矿用液压移动列车组单车","4000mm*1400mm","台",18]
[1.2,"矿用液压移动列车组单车","4500mm*1400mm","台",4]
[1.3,"矿用液压移动列车组单车","6000mm*1400mm","台",10]
[2,"电缆桥架车存储装置",null,"套",1,"存缆量不得少于30米，不少于16辆缆车。"]
[3,"电液控制系统",null,"套","---","自移设备列车电液控系统选用四川航天产品、各控制传感器由列车厂家提供，并负责安装，实现自动化控制。"]
[4,"专用工具",null,"套",2]
[5,"随机技术资料",null,"套","6+1","每套配（含一套电子版）"]
[6,"列车专用泵站（含液箱）",null,"套",1,"需满足列车系统压力要求。"]
[null,"供电电压等级为660V/1140V"]
["备注：设备列车电缆架全部塑封，顶部设计全封闭电缆槽水管槽。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}